# *ANNEX II + III:* TECHNICAL SPECIFICATIONS + TECHNICAL OFFER

**Contract title:Supply of LED display (LOT 2) p 1 /1**

**Publication reference:**CB007.2.13.173/TD1

**Columns 1-2 should be completed by the contracting authority**

**Columns 3-4 should be completed by the tenderer**

**Column 5 is reserved for the evaluation committee**

Annex III - the contractor's technical offer

The tenderers are requested to complete the template on the next pages:

* Column 2 is completed by the contracting authority shows the required specifications (not to be modified by the tenderer),
* Column 3 is to be filled in by the tenderer and must detail what is offered (for example the words ‘compliant’ or ‘yes’ are not sufficient)
* Column 4 allows the tenderer to make comments onits proposed supply and to make eventual references to the documentation

The eventual documentation supplied should clearly indicate (highlight, mark) the models offered and the options included, if any, so that the evaluators can see the exact configuration. Offers that do not permit to identify precisely the models and the specifications may be rejected by the evaluation committee.

The offer must be clear enough to allow the evaluators to make an easy comparison between the requested specifications and the offeredspecifications.

| **1.****Item number** | **2.****Specificationsrequired** | **3.****Specificationsoffered** | **4.****Notes, remarks, ref to documentation** | **5.****Evaluation committee’s notes**  |
| --- | --- | --- | --- | --- |
| 1 | **LED display (4800mm\*2880mm)**External use: YesOverall size:  4800mm x 2880mmCabinet size:  960 x 960 mmBrightness: ≥ 7500 cdViewing angle: ≥ 120 ° Horizontal 120 ° VerticalRefresh rate: ≥ 1920hzDamage rate: <0.0001Operating temperature: 25°C ῀ 65°C |  |  |  |